|  |
| --- |
| **Blowing Machine Comparative Matrix**  |
|   |  |
|

|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
| Feature  | Volu-Matic® V  | Volu-Matic® IV  | Volu-Matic® III  | Volu-Matic® SE  | Volu-Matic® MS  | Attic-Mattic™  | Multi-Matic™  |
| Positive Displacement Blower  | Std  | Std  | Std  | Std  | Std  | Std  | Std  |
| Air Bleed System  | Std  | N/A  | Std  | Std  | Std  | Std  | N/A  |
| 4-Speed Transmission  | Std  | N/A  | Std  | Std  | N/A  | N/A  | N/A  |
| Material Control Slide  | Std  | Std  | Std  | Std  | Std  | Std  | Std  |
| Self-Aligning Sealed Bearings  | Std  | Std  | Std  | Std  | Std  | Std  | Std  |
| Heavy-Duty Gearboxes  | Std  | N/A  | Std  | N/A  | N/A  | N/A  | Std  |
| Heavy-Duty Electric Clutches  | Std  | N/A  | Std  | N/A  | N/A  | N/A  | N/A  |
| Automatic Back Flow Check Valve  | Std  | Std  | Std  | Std  | Std  | Std  | Std  |
| Electrical Overload Protection  | Std  | Std  | Std  | Std  | Std  | Std  | Std  |
| Mechanical Overload Protection  | Std  | Std  | Std  | Std  | N/A  | Std  | Std  |
| Automatic Pressure Relief Valve  | Std  | Std  | Std  | N/A  | N/A  | N/A  | N/A  |
| Quick-Change Seal System  | Opt  | Std  | Opt  | N/A  | N/A  | N/A  | N/A  |
| Integrated Safety Features  | Std  | Std  | Std  | Std  | Std  | Std  | Std  |
| Adjustable Drive Belts  | Std  | Std  | Std  | Std  | Std  | Std  | Std  |
| Expanded Hopper  | Std  | Opt  | Opt  | Opt  | N/A  | Opt  | Std  |
| Built-In Water Pump  | Std  | Opt  | Opt  | N/A  | N/A  | Opt  | \*  |
| Integrated Vacuum System  | Std  | N/A  | N/A  | N/A  | N/A  | N/A  | Std  |
| Fully Hydraulic Drive System  | N/A  | Std  | N/A  | N/A  | N/A  | N/A  | Std  |
| Wired Remote Control  | Std  | Std  | Std  | Std  | Std  | Std  | Std  |
| Wireless Remote Control  | Opt  | Opt  | Opt  | Opt  | Opt  | Opt  | Opt  |
| Power Sources  |
|      PTO Driven  | Std  | Opt  | Opt  | Opt  | N/A  | Opt  | Std  |
|      Engine Driven  | N/A  | Opt  | Opt  | Opt  | Std  | Opt  | N/A  |
|      Electric  | N/A  | Opt  | Opt  | N/A  | N/A  | Opt  | N/A  |
| Physical Dimensions  |
|      Height - Inches / (cm)  | 88 / (224)  | 73 / (186)  | 74 / (188)  | 69 / (175)  | 68 / (173)  | 67 / (170)  | 95 / (241)  |
|      Width  | 80 / (203)  | 83 / (211)  | 75 / (191)  | 72 / (183)  | 54 / (137)  | 75 / (191)  | 84.5 / (214)  |
|      Depth  | 88.5 / (225)  | 56.5 / (144)  | 56.5 / (144)  | 48 / (122)  | 46.5 / (118)  | 48 / (122)  | 80 / (203)  |
|      Weight - lbs / (kg)  | 2500 / (1134)  | 2100 / (952)  | 2000 / (907)  | 1300 / (590)  | 850 / (385)  | 1480 / (671)  | 3100 / (1406)  |
| Open Blow Output (lbs/min)  |
|      Fiberglass  | 25-35  | 25-35  | 25-35  | 25-35  | 11-15  | 15-20  | N/A  |
|      Rockwool  | 35-55  | 35-55  | 35-55  | 35-55  | 16-22  | 25-30  | N/A  |
|      Cellulose  | 70-80  | 70-80  | 70-80  | 70-80  | 15-20  | 30-50  | 14-20\*\*  |
| Applications  |
|      Open Blow  | Yes  | Yes  | Yes  | Yes  | Yes  | Yes  | N/A  |
|      Side Wall Spray  | Yes  | Yes  | Yes  | No  | No  | Yes  | Yes  |
|      Dense Pack / Cavity Fill  | Yes  | Yes  | Yes  | Yes  | Yes  | Yes  | Yes  |

Std - Standard feature Opt - Optional Feature N/A - Feature not available on this model \* Water pump is an integral part of the Multi-Tank water system required for this model \*\* Machine specifically designed for cellulose Side Wall Spray and Dense Pack / Cavity Fill applications |