|  |  |
| --- | --- |
| **Blowing Machine Comparative Matrix** | |
|  |  |
| |  |  |  |  |  |  |  |  | | --- | --- | --- | --- | --- | --- | --- | --- | | Feature | Volu-Matic® V | Volu-Matic® IV | Volu-Matic® III | Volu-Matic® SE | Volu-Matic® MS | Attic-Mattic™ | Multi-Matic™ | | Positive Displacement Blower | Std | Std | Std | Std | Std | Std | Std | | Air Bleed System | Std | N/A | Std | Std | Std | Std | N/A | | 4-Speed Transmission | Std | N/A | Std | Std | N/A | N/A | N/A | | Material Control Slide | Std | Std | Std | Std | Std | Std | Std | | Self-Aligning Sealed Bearings | Std | Std | Std | Std | Std | Std | Std | | Heavy-Duty Gearboxes | Std | N/A | Std | N/A | N/A | N/A | Std | | Heavy-Duty Electric Clutches | Std | N/A | Std | N/A | N/A | N/A | N/A | | Automatic Back Flow Check Valve | Std | Std | Std | Std | Std | Std | Std | | Electrical Overload Protection | Std | Std | Std | Std | Std | Std | Std | | Mechanical Overload Protection | Std | Std | Std | Std | N/A | Std | Std | | Automatic Pressure Relief Valve | Std | Std | Std | N/A | N/A | N/A | N/A | | Quick-Change Seal System | Opt | Std | Opt | N/A | N/A | N/A | N/A | | Integrated Safety Features | Std | Std | Std | Std | Std | Std | Std | | Adjustable Drive Belts | Std | Std | Std | Std | Std | Std | Std | | Expanded Hopper | Std | Opt | Opt | Opt | N/A | Opt | Std | | Built-In Water Pump | Std | Opt | Opt | N/A | N/A | Opt | \* | | Integrated Vacuum System | Std | N/A | N/A | N/A | N/A | N/A | Std | | Fully Hydraulic Drive System | N/A | Std | N/A | N/A | N/A | N/A | Std | | Wired Remote Control | Std | Std | Std | Std | Std | Std | Std | | Wireless Remote Control | Opt | Opt | Opt | Opt | Opt | Opt | Opt | | Power Sources | | | | | | | | | PTO Driven | Std | Opt | Opt | Opt | N/A | Opt | Std | | Engine Driven | N/A | Opt | Opt | Opt | Std | Opt | N/A | | Electric | N/A | Opt | Opt | N/A | N/A | Opt | N/A | | Physical Dimensions | | | | | | | | | Height - Inches / (cm) | 88 / (224) | 73 / (186) | 74 / (188) | 69 / (175) | 68 / (173) | 67 / (170) | 95 / (241) | | Width | 80 / (203) | 83 / (211) | 75 / (191) | 72 / (183) | 54 / (137) | 75 / (191) | 84.5 / (214) | | Depth | 88.5 / (225) | 56.5 / (144) | 56.5 / (144) | 48 / (122) | 46.5 / (118) | 48 / (122) | 80 / (203) | | Weight - lbs / (kg) | 2500 / (1134) | 2100 / (952) | 2000 / (907) | 1300 / (590) | 850 / (385) | 1480 / (671) | 3100 / (1406) | | Open Blow Output (lbs/min) | | | | | | | | | Fiberglass | 25-35 | 25-35 | 25-35 | 25-35 | 11-15 | 15-20 | N/A | | Rockwool | 35-55 | 35-55 | 35-55 | 35-55 | 16-22 | 25-30 | N/A | | Cellulose | 70-80 | 70-80 | 70-80 | 70-80 | 15-20 | 30-50 | 14-20\*\* | | Applications | | | | | | | | | Open Blow | Yes | Yes | Yes | Yes | Yes | Yes | N/A | | Side Wall Spray | Yes | Yes | Yes | No | No | Yes | Yes | | Dense Pack / Cavity Fill | Yes | Yes | Yes | Yes | Yes | Yes | Yes |   Std - Standard feature  Opt - Optional Feature  N/A - Feature not available on this model  \* Water pump is an integral part of the Multi-Tank water system required for this model  \*\* Machine specifically designed for cellulose Side Wall Spray and Dense Pack / Cavity Fill applications | |